Pivot hinge: FritsJurgens System One - MPDS-FO WS serie -
Dimensions (thickness x height x width) 32 x 39 x 160 mm
Minimal door thickness: 40 mm
Weight capacity: 0 - 500 kg
Depth in doors: 40 mm
No hold positions, not self-closing, no adjustable door movement
Axial adjustment +/- 5 mm
 
A pivot hinge set System One consists of:
1 piece pivot hinge System One integrated in the door, made of hardened stainless steel and anodized aluminum.        
1 piece top pivot: integrated in the door (except Top pivot Reversed, which is mounted in the frame or ceiling), made of stainless steel. Equipped with a hardened pin to be rotated upwards into the iglidur bearing in the ceiling plate. The axial direction is adjustable +/- 5 mm.
1 piece floor plate: mounted on the floor, made of hardened stainless steel, and provided with an oval tapered recess for the fitting of the uniform base of the pivot hinge.
1 piece ceiling plate: mounted in the ceiling, made of stainless steel, and provided with an iglidur bearing for mounting the uniform pin in the top pivot.
1 piece Allen wrench 5 mm, for adjustment of the top pivot.
1 piece fitting template for mounting the floor plate.
1 tube fitting adhesive for mounting the floor and ceiling plate.
1 set of screws for mounting the pivot hinge, System One, and the ceiling plate.
 
2-year warranty (see terms and conditions).
 
Pivot point: fixed at 40 mm or adjustable from 70 mm up to the middle of the door (depending on the top pivot of your choice). 
 
For door dimensions/weight and top pivot options, use the FritsJurgens Selector: www.fritsjurgens.com/selector